**nRF Connect, 2021-10-24**

**DFU\_RstatEasySmart (EC:35:2B:48:C3:F2)**

11:22:27.322 Connecting to EC:35:2B:48:C3:F2...

11:22:27.328 gatt = device.connectGatt(autoConnect = false, TRANSPORT\_LE, preferred PHY = LE 1M)

11:22:28.395 [Broadcast] Action received: android.bluetooth.device.action.ACL\_CONNECTED

11:22:28.421 [Callback] Connection state changed with status: 0 and new state: CONNECTED (2)

11:22:28.421 Connected to EC:35:2B:48:C3:F2

11:22:28.455 Discovering services...

11:22:28.455 gatt.discoverServices()

11:22:28.836 Connection parameters updated (interval: 7.5ms, latency: 0, timeout: 5000ms)

11:22:28.995 [Callback] Services discovered with status: 0

11:22:28.995 Services discovered

11:22:29.023 Generic Access (0x1800)

- Device Name [R W] (0x2A00)

- Appearance [R] (0x2A01)

- Peripheral Preferred Connection Parameters [R] (0x2A04)

- Central Address Resolution [R] (0x2AA6)

Generic Attribute (0x1801)

- Service Changed [I] (0x2A05)

   Client Characteristic Configuration (0x2902)

Secure DFU Service (0xFE59)

- DFU Packet [WNR] (8ec90002-f315-4f60-9fb8-838830daea50)

- DFU Control Point [N W] (8ec90001-f315-4f60-9fb8-838830daea50)

   Client Characteristic Configuration (0x2902)

11:22:29.024 gatt.setCharacteristicNotification(00002a05-0000-1000-8000-00805f9b34fb, true)

11:22:29.107 Connection parameters updated (interval: 45.0ms, latency: 0, timeout: 5000ms)

11:22:39.831 [DFU] DFU service started

11:22:39.831 [DFU] Opening file...

11:22:39.831 [DFU] Firmware file opened successfully

11:22:39.831 [DFU] Connecting to DFU target...

11:22:39.831 [DFU] gatt = device.connectGatt(autoConnect = false, TRANSPORT\_LE, preferredPhy = LE\_1M | LE\_2M)

11:22:39.833 [DFU] Connected to EC:35:2B:48:C3:F2

11:22:39.835 [DFU] Discovering services...

11:22:39.835 [DFU] gatt.discoverServices()

11:22:39.837 [DFU] Services discovered

11:22:39.853 [DFU] wait(1000)

11:22:40.863 [DFU] Requesting new MTU...

11:22:40.863 [DFU] gatt.requestMtu(517)

11:22:40.939 [DFU] MTU changed to: 23

11:22:40.939 [DFU] Enabling notifications for 8ec90001-f315-4f60-9fb8-838830daea50

11:22:40.939 [DFU] gatt.setCharacteristicNotification(8ec90001-f315-4f60-9fb8-838830daea50, true)

11:22:40.941 [DFU] gatt.writeDescriptor(00002902-0000-1000-8000-00805f9b34fb, value=0x01-00)

11:22:41.030 [DFU] Data written to descr.8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **01-00**

11:22:41.030 [DFU] Notifications enabled for 8ec90001-f315-4f60-9fb8-838830daea50

11:22:41.030 [DFU] Notifications enabled

11:22:41.030 [DFU] wait(1000)

11:22:42.032 [DFU] Writing to characteristic 8ec90001-f315-4f60-9fb8-838830daea50

11:22:42.032 [DFU] gatt.writeCharacteristic(8ec90001-f315-4f60-9fb8-838830daea50)

11:22:42.115 [DFU] Notification received from 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-06-01-00-01-00-00-00-00-00-00-00-00-00-00**

11:22:42.116 [DFU] Data written to 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-06-01-00-01-00-00-00-00-00-00-00-00-00-00**

11:22:42.117 [DFU] Command object info received (**Max size = 256, Offset = 0, CRC = 00000000**)

11:22:42.117 [DFU] Writing to characteristic 8ec90001-f315-4f60-9fb8-838830daea50

11:22:42.117 [DFU] gatt.writeCharacteristic(8ec90001-f315-4f60-9fb8-838830daea50)

11:22:42.201 [DFU] Notification received from 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-02-01**

11:22:42.201 [DFU] Data written to 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-02-01**

11:22:42.203 [DFU] Packet Receipt Notif disabled (**Op Code = 2, Value = 0**)

11:22:42.203 [DFU] Writing to characteristic 8ec90001-f315-4f60-9fb8-838830daea50

11:22:42.203 [DFU] gatt.writeCharacteristic(8ec90001-f315-4f60-9fb8-838830daea50)

11:22:42.294 [DFU] Notification received from 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-01-01**

11:22:42.295 [DFU] Data written to 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-01-01**

11:22:42.296 [DFU] Command object created

11:22:42.296 [DFU] Writing to characteristic 8ec90002-f315-4f60-9fb8-838830daea50

11:22:42.296 [DFU] gatt.writeCharacteristic(8ec90002-f315-4f60-9fb8-838830daea50)

11:22:42.302 [DFU] Data written to 8ec90002-f315-4f60-9fb8-838830daea50, value (0x): **12-84-01-0A-3E-08-01-12-3A-08-04-10-34-1A-02-9D-01-20-00-28**

11:22:42.303 [DFU] Writing to characteristic 8ec90002-f315-4f60-9fb8-838830daea50

11:22:42.303 [DFU] gatt.writeCharacteristic(8ec90002-f315-4f60-9fb8-838830daea50)

11:22:42.315 [DFU] Data written to 8ec90002-f315-4f60-9fb8-838830daea50, value (0x): **00-30-00-38-E8-8C-02-42-24-08-03-12-20-58-E1-29-33-52-06-48**

11:22:42.318 [DFU] Writing to characteristic 8ec90002-f315-4f60-9fb8-838830daea50

11:22:42.318 [DFU] gatt.writeCharacteristic(8ec90002-f315-4f60-9fb8-838830daea50)

11:22:42.325 [DFU] Data written to 8ec90002-f315-4f60-9fb8-838830daea50, value (0x): **1E-A9-36-FF-04-EB-3A-44-82-2E-F7-E1-C3-17-62-4D-B1-3E-D5-68**

11:22:42.329 [DFU] Writing to characteristic 8ec90002-f315-4f60-9fb8-838830daea50

11:22:42.337 [DFU] gatt.writeCharacteristic(8ec90002-f315-4f60-9fb8-838830daea50)

11:22:42.343 [DFU] Data written to 8ec90002-f315-4f60-9fb8-838830daea50, value (0x): **CA-AF-E0-89-AB-48-00-10-00-1A-40-DD-33-AC-E6-A1-6B-AD-D8-E0**

11:22:42.343 [DFU] Writing to characteristic 8ec90002-f315-4f60-9fb8-838830daea50

11:22:42.343 [DFU] gatt.writeCharacteristic(8ec90002-f315-4f60-9fb8-838830daea50)

11:22:42.348 [DFU] Data written to 8ec90002-f315-4f60-9fb8-838830daea50, value (0x): **C7-0A-4C-53-E4-A6-B1-5D-4B-D4-0C-07-D9-0C-71-F3-9D-EB-6F-CB**

11:22:42.349 [DFU] Writing to characteristic 8ec90002-f315-4f60-9fb8-838830daea50

11:22:42.349 [DFU] gatt.writeCharacteristic(8ec90002-f315-4f60-9fb8-838830daea50)

11:22:42.353 [DFU] Data written to 8ec90002-f315-4f60-9fb8-838830daea50, value (0x): **E2-CC-33-9E-F0-AA-46-56-5A-3B-5A-20-CF-05-84-8F-4B-3A-02-76**

11:22:42.354 [DFU] Writing to characteristic 8ec90002-f315-4f60-9fb8-838830daea50

11:22:42.354 [DFU] gatt.writeCharacteristic(8ec90002-f315-4f60-9fb8-838830daea50)

11:22:42.363 [DFU] Data written to 8ec90002-f315-4f60-9fb8-838830daea50, value (0x): **59-FB-4F-ED-AC-6A-AF-7D-E8-3A-C8-3C-41-81-22**

11:22:42.364 [DFU] Command object sent (CRC = 8854858F)

11:22:42.364 [DFU] Writing to characteristic 8ec90001-f315-4f60-9fb8-838830daea50

11:22:42.364 [DFU] gatt.writeCharacteristic(8ec90001-f315-4f60-9fb8-838830daea50)

11:22:42.427 [DFU] Notification received from 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-03-01-87-00-00-00-8F-85-54-88**

11:22:42.428 [DFU] Data written to 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-03-01-87-00-00-00-8F-85-54-88**

11:22:42.430 [DFU] Checksum received (Offset = 135, CRC = 8854858F)

11:22:42.431 [DFU] Writing to characteristic 8ec90001-f315-4f60-9fb8-838830daea50

11:22:42.431 [DFU] gatt.writeCharacteristic(8ec90001-f315-4f60-9fb8-838830daea50)

11:22:42.518 [DFU] Data written to 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **04**

11:22:42.653 [DFU] Notification received from 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-04-01**

11:22:42.656 [DFU] Command object executed

11:22:42.656 [DFU] Writing to characteristic 8ec90001-f315-4f60-9fb8-838830daea50

11:22:42.656 [DFU] gatt.writeCharacteristic(8ec90001-f315-4f60-9fb8-838830daea50)

11:22:42.833 [DFU] Notification received from 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-02-01**

11:22:42.834 [DFU] Data written to 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-02-01**

11:22:42.836 [DFU] Packet Receipt Notif Req (Op Code = 2) sent (Value = 10)

11:22:42.836 [DFU] Writing to characteristic 8ec90001-f315-4f60-9fb8-838830daea50

11:22:42.836 [DFU] gatt.writeCharacteristic(8ec90001-f315-4f60-9fb8-838830daea50)

11:22:42.932 [DFU] Notification received from 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-06-01-00-10-00-00-00-00-00-00-00-00-00-00**

11:22:42.932 [DFU] Data written to 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-06-01-00-10-00-00-00-00-00-00-00-00-00-00**

11:22:42.932 [DFU] Data object info received (**Max size = 4096, Offset = 0, CRC = 00000000**)

11:22:42.978 [DFU] Writing to characteristic 8ec90001-f315-4f60-9fb8-838830daea50

11:22:42.978 [DFU] gatt.writeCharacteristic(8ec90001-f315-4f60-9fb8-838830daea50)

11:22:43.010 [DFU] Notification received from 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-01-01**

11:22:43.011 [DFU] Data written to 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-01-01**

11:22:43.011 [DFU] Data object (1/9) created

11:22:43.011 [DFU] wait(400)

11:22:43.412 [DFU] Uploading firmware...

11:22:43.412 [DFU] Sending firmware to characteristic 8ec90002-f315-4f60-9fb8-838830daea50...

11:22:46.221 [DFU] Writing to characteristic 8ec90001-f315-4f60-9fb8-838830daea50

11:22:46.221 [DFU] gatt.writeCharacteristic(8ec90001-f315-4f60-9fb8-838830daea50)

11:22:46.341 [DFU] Notification received from 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-03-01-00-10-00-00-E8-68-30-D5**

11:22:46.341 [DFU] Data written to 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-03-01-00-10-00-00-E8-68-30-D5**

11:22:46.344 [DFU] Checksum received (**Offset = 4096, CRC = D53068E8**)

11:22:46.344 [DFU] Writing to characteristic 8ec90001-f315-4f60-9fb8-838830daea50

11:22:46.344 [DFU] gatt.writeCharacteristic(8ec90001-f315-4f60-9fb8-838830daea50)

11:22:46.432 [DFU] Notification received from 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-04-01**

11:22:46.437 [DFU] Data written to 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-04-01**

11:22:46.437 [DFU] Data object executed

11:22:46.437 [DFU] Writing to characteristic 8ec90001-f315-4f60-9fb8-838830daea50

11:22:46.437 [DFU] gatt.writeCharacteristic(8ec90001-f315-4f60-9fb8-838830daea50)

11:22:46.611 [DFU] Notification received from 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-01-01**

11:22:46.612 [DFU] Data written to 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-01-01**

11:22:46.612 [DFU] Data object (2/9) created

11:22:46.612 [DFU] wait(400)

11:22:47.016 [DFU] Uploading firmware...

11:22:47.027 [DFU] Sending firmware to characteristic 8ec90002-f315-4f60-9fb8-838830daea50...

11:22:49.823 [DFU] Writing to characteristic 8ec90001-f315-4f60-9fb8-838830daea50

11:22:49.823 [DFU] gatt.writeCharacteristic(8ec90001-f315-4f60-9fb8-838830daea50)

11:22:49.941 [DFU] Notification received from 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-03-01-00-20-00-00-5A-B2-7B-6D**

11:22:49.942 [DFU] Data written to 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-03-01-00-20-00-00-5A-B2-7B-6D**

11:22:49.942 [DFU] Checksum received (**Offset = 8192, CRC = 6D7BB25A**)

11:22:49.942 [DFU] Writing to characteristic 8ec90001-f315-4f60-9fb8-838830daea50

11:22:49.943 [DFU] gatt.writeCharacteristic(8ec90001-f315-4f60-9fb8-838830daea50)

11:22:50.035 [DFU] Notification received from 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-04-01**

11:22:50.039 [DFU] Data written to 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-04-01**

11:22:50.039 [DFU] Data object executed

11:22:50.039 [DFU] Writing to characteristic 8ec90001-f315-4f60-9fb8-838830daea50

11:22:50.039 [DFU] gatt.writeCharacteristic(8ec90001-f315-4f60-9fb8-838830daea50)

11:22:50.212 [DFU] Notification received from 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-01-01**

11:22:50.212 [DFU] Data written to 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-01-01**

11:22:50.213 [DFU] Data object (3/9) created

11:22:50.213 [DFU] wait(400)

11:22:50.617 [DFU] Uploading firmware...

11:22:50.617 [DFU] Sending firmware to characteristic 8ec90002-f315-4f60-9fb8-838830daea50...

11:22:53.376 [DFU] Writing to characteristic 8ec90001-f315-4f60-9fb8-838830daea50

11:22:53.376 [DFU] gatt.writeCharacteristic(8ec90001-f315-4f60-9fb8-838830daea50)

11:22:53.502 [DFU] Notification received from 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-03-01-00-30-00-00-3E-F7-88-62**

11:22:53.503 [DFU] Data written to 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-03-01-00-30-00-00-3E-F7-88-62**

11:22:53.507 [DFU] Checksum received (**Offset = 12288, CRC = 6288F73E**)

11:22:53.507 [DFU] Writing to characteristic 8ec90001-f315-4f60-9fb8-838830daea50

11:22:53.507 [DFU] gatt.writeCharacteristic(8ec90001-f315-4f60-9fb8-838830daea50)

11:22:53.592 [DFU] Notification received from 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-04-01**

11:22:53.594 [DFU] Data written to 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-04-01**

11:22:53.595 [DFU] Data object executed

11:22:53.595 [DFU] Writing to characteristic 8ec90001-f315-4f60-9fb8-838830daea50

11:22:53.595 [DFU] gatt.writeCharacteristic(8ec90001-f315-4f60-9fb8-838830daea50)

11:22:53.768 [DFU] Notification received from 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-01-01**

11:22:53.769 [DFU] Data written to 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-01-01**

11:22:53.769 [DFU] Data object (4/9) created

11:22:53.770 [DFU] wait(400)

11:22:54.173 [DFU] Uploading firmware...

11:22:54.175 [DFU] Sending firmware to characteristic 8ec90002-f315-4f60-9fb8-838830daea50...

11:22:56.933 [DFU] Writing to characteristic 8ec90001-f315-4f60-9fb8-838830daea50

11:22:56.933 [DFU] gatt.writeCharacteristic(8ec90001-f315-4f60-9fb8-838830daea50)

11:22:57.055 [DFU] Notification received from 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-03-01-00-40-00-00-53-35-C0-E7**

11:22:57.055 [DFU] Data written to 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-03-01-00-40-00-00-53-35-C0-E7**

11:22:57.056 [DFU] Checksum received (**Offset = 16384, CRC = E7C03553**)

11:22:57.056 [DFU] Writing to characteristic 8ec90001-f315-4f60-9fb8-838830daea50

11:22:57.056 [DFU] gatt.writeCharacteristic(8ec90001-f315-4f60-9fb8-838830daea50)

11:22:57.143 [DFU] Notification received from 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-04-01**

11:22:57.148 [DFU] Data written to 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-04-01**

11:22:57.148 [DFU] Data object executed

11:22:57.148 [DFU] Writing to characteristic 8ec90001-f315-4f60-9fb8-838830daea50

11:22:57.148 [DFU] gatt.writeCharacteristic(8ec90001-f315-4f60-9fb8-838830daea50)

11:22:57.323 [DFU] Notification received from 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-01-01**

11:22:57.323 [DFU] Data written to 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-01-01**

11:22:57.324 [DFU] Data object (5/9) created

11:22:57.324 [DFU] wait(400)

11:22:57.725 [DFU] Uploading firmware...

11:22:57.726 [DFU] Sending firmware to characteristic 8ec90002-f315-4f60-9fb8-838830daea50...

11:23:00.581 [DFU] Writing to characteristic 8ec90001-f315-4f60-9fb8-838830daea50

11:23:00.581 [DFU] gatt.writeCharacteristic(8ec90001-f315-4f60-9fb8-838830daea50)

11:23:00.699 [DFU] Notification received from 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-03-01-00-50-00-00-E3-33-02-F6**

11:23:00.699 [DFU] Data written to 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-03-01-00-50-00-00-E3-33-02-F6**

11:23:00.703 [DFU] Checksum received (**Offset = 20480, CRC = F60233E3**)

11:23:00.712 [DFU] Writing to characteristic 8ec90001-f315-4f60-9fb8-838830daea50

11:23:00.716 [DFU] gatt.writeCharacteristic(8ec90001-f315-4f60-9fb8-838830daea50)

11:23:00.784 [DFU] Notification received from 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-04-01**

11:23:00.784 [DFU] Data written to 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-04-01**

11:23:00.784 [DFU] Data object executed

11:23:00.784 [DFU] Writing to characteristic 8ec90001-f315-4f60-9fb8-838830daea50

11:23:00.785 [DFU] gatt.writeCharacteristic(8ec90001-f315-4f60-9fb8-838830daea50)

11:23:00.964 [DFU] Notification received from 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-01-01**

11:23:00.965 [DFU] Data written to 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-01-01**

11:23:00.965 [DFU] Data object (6/9) created

11:23:00.965 [DFU] wait(400)

11:23:01.368 [DFU] Uploading firmware...

11:23:01.368 [DFU] Sending firmware to characteristic 8ec90002-f315-4f60-9fb8-838830daea50...

11:23:04.171 [DFU] Writing to characteristic 8ec90001-f315-4f60-9fb8-838830daea50

11:23:04.171 [DFU] gatt.writeCharacteristic(8ec90001-f315-4f60-9fb8-838830daea50)

11:23:04.296 [DFU] Notification received from 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-03-01-00-60-00-00-F3-80-A1-69**

11:23:04.296 [DFU] Data written to 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-03-01-00-60-00-00-F3-80-A1-69**

11:23:04.297 [DFU] Checksum received (**Offset = 24576, CRC = 69A180F3**)

11:23:04.297 [DFU] Writing to characteristic 8ec90001-f315-4f60-9fb8-838830daea50

11:23:04.297 [DFU] gatt.writeCharacteristic(8ec90001-f315-4f60-9fb8-838830daea50)

11:23:04.387 [DFU] Notification received from 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-04-01**

11:23:04.387 [DFU] Data written to 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-04-01**

11:23:04.387 [DFU] Data object executed

11:23:04.387 [DFU] Writing to characteristic 8ec90001-f315-4f60-9fb8-838830daea50

11:23:04.387 [DFU] gatt.writeCharacteristic(8ec90001-f315-4f60-9fb8-838830daea50)

11:23:04.567 [DFU] Notification received from 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-01-01**

11:23:04.568 [DFU] Data written to 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-01-01**

11:23:04.568 [DFU] Data object (7/9) created

11:23:04.571 [DFU] wait(400)

11:23:04.972 [DFU] Uploading firmware...

11:23:04.972 [DFU] Sending firmware to characteristic 8ec90002-f315-4f60-9fb8-838830daea50...

11:23:07.821 [DFU] Writing to characteristic 8ec90001-f315-4f60-9fb8-838830daea50

11:23:07.821 [DFU] gatt.writeCharacteristic(8ec90001-f315-4f60-9fb8-838830daea50)

11:23:07.943 [DFU] Notification received from 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-03-01-00-70-00-00-CF-27-9F-A7**

11:23:07.945 [DFU] Data written to 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-03-01-00-70-00-00-CF-27-9F-A7**

11:23:07.951 [DFU] Checksum received (**Offset = 28672, CRC = A79F27CF**)

11:23:07.956 [DFU] Writing to characteristic 8ec90001-f315-4f60-9fb8-838830daea50

11:23:07.958 [DFU] gatt.writeCharacteristic(8ec90001-f315-4f60-9fb8-838830daea50)

11:23:08.036 [DFU] Notification received from 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-04-01**

11:23:08.037 [DFU] Data written to 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-04-01**

11:23:08.037 [DFU] Data object executed

11:23:08.038 [DFU] Writing to characteristic 8ec90001-f315-4f60-9fb8-838830daea50

11:23:08.038 [DFU] gatt.writeCharacteristic(8ec90001-f315-4f60-9fb8-838830daea50)

11:23:08.213 [DFU] Notification received from 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-01-01**

11:23:08.214 [DFU] Data written to 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-01-01**

11:23:08.221 [DFU] Data object (8/9) created

11:23:08.221 [DFU] wait(400)

11:23:08.615 [DFU] Uploading firmware...

11:23:08.615 [DFU] Sending firmware to characteristic 8ec90002-f315-4f60-9fb8-838830daea50...

11:23:11.412 [DFU] Writing to characteristic 8ec90001-f315-4f60-9fb8-838830daea50

11:23:11.412 [DFU] gatt.writeCharacteristic(8ec90001-f315-4f60-9fb8-838830daea50)

11:23:11.499 [DFU] Data written to 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **03**

11:23:11.500 [DFU] Notification received from 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-03-01-00-80-00-00-A5-68-E4-65**

11:23:11.500 [DFU] Checksum received (**Offset = 32768, CRC = 65E468A5**)

11:23:11.500 [DFU] Writing to characteristic 8ec90001-f315-4f60-9fb8-838830daea50

11:23:11.500 [DFU] gatt.writeCharacteristic(8ec90001-f315-4f60-9fb8-838830daea50)

11:23:11.587 [DFU] Notification received from 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-04-01**

11:23:11.587 [DFU] Data written to 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-04-01**

11:23:11.588 [DFU] Data object executed

11:23:11.588 [DFU] Writing to characteristic 8ec90001-f315-4f60-9fb8-838830daea50

11:23:11.588 [DFU] gatt.writeCharacteristic(8ec90001-f315-4f60-9fb8-838830daea50)

11:23:11.768 [DFU] Notification received from 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-01-01**

11:23:11.768 [DFU] Data written to 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-01-01**

11:23:11.770 [DFU] Data object (9/9) created

11:23:11.773 [DFU] wait(400)

11:23:12.173 [DFU] Uploading firmware...

11:23:12.173 [DFU] Sending firmware to characteristic 8ec90002-f315-4f60-9fb8-838830daea50...

11:23:13.307 [DFU] Writing to characteristic 8ec90001-f315-4f60-9fb8-838830daea50

11:23:13.307 [DFU] gatt.writeCharacteristic(8ec90001-f315-4f60-9fb8-838830daea50)

11:23:13.340 [DFU] Notification received from 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-03-01-68-86-00-00-2C-20-01-3B**

11:23:13.342 [DFU] Data written to 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-03-01-68-86-00-00-2C-20-01-3B**

11:23:13.342 [DFU] Checksum received (**Offset = 34408, CRC = 3B01202C**)

11:23:13.342 [DFU] Writing to characteristic 8ec90001-f315-4f60-9fb8-838830daea50

11:23:13.342 [DFU] gatt.writeCharacteristic(8ec90001-f315-4f60-9fb8-838830daea50)

11:23:13.430 [DFU] Data written to 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **04**

11:23:13.481 [DFU] Notification received from 8ec90001-f315-4f60-9fb8-838830daea50, value (0x): **60-04-01**

11:23:13.481 [DFU] Data object executed

11:23:13.481 [DFU] Upload completed in 30542 ms

11:23:13.704 [Callback] Connection state changed with status: 19 and new state: DISCONNECTED (0)

11:23:13.704 Connection terminated by peer (status 19)

11:23:13.704 Disconnected

11:23:13.749 [DFU] Disconnected by the remote device

11:23:13.749 [DFU] gatt.refresh() (hidden)

11:23:13.749 [DFU] gatt.disconnect()

11:23:13.749 [DFU] gatt.close()

11:23:13.749 [DFU] wait(1400)

11:23:13.750 [Broadcast] Action received: android.bluetooth.device.action.ACL\_DISCONNECTED

11:23:13.774 [DFU] [Broadcast] Action received: android.bluetooth.device.action.ACL\_DISCONNECTED

11:23:15.155 gatt.close()

11:23:15.156 wait(200)

11:23:15.358 Connecting to EC:35:2B:48:C3:F2...

11:23:15.358 gatt = device.connectGatt(autoConnect = false, TRANSPORT\_LE, preferred PHY = LE 1M)

11:23:18.122 Cancelling connection...

11:23:18.122 gatt.disconnect()

11:23:18.123 Disconnected